SEQ2ZMX v 1.3  

  Utility to convert Code V(TM) sequence files to ZEMAX files

  Syntax:

  SEQ2ZMX  INPUTFILENAME OUTPUTFILENAME LOGFILENAME

  Where
  INPUTFILENAME is the input sequence file name, i.e. LENS.SEQ
  OUTPUTFILENAME is the output ZEMAX file name, i.e. LENS.ZMX
  LOGFILENAME is the optional log file name. Default = seq2zmx.LOG
  File names may include the drive and path.

  Supported Commands:

  Aspheric surface type
  Conic surface type		
  Cylindrical surface type
  Grating surface type
  Spherical surface type
  Default dimensions
  Numerical aperture, F/#
  PIM solve
  Radius or curvature, thickness, glass
  Wavelengths, reference wavelength, and weights
  Field angles, object height, and paraxial image height
  Title
  X,Y,Z tilts, decenters, BEN and DAR commands
  Zooms on thickness

  Disclaimer:
  This utility is provided as is without warranty either expressed or implied.
  The utility is intended to convert simple Code V ver. 8.1 sequence files to
  ZEMAX lens files. Not all Code V commands are supported. Complex systems
  may require additional editing within ZEMAX. Unconverted commands
  are stored in the log file. E-mail conversion suggestions to
  support@zemax.com .

